[to index] | [close window] | [C_SHORT Verification]

# Coplanar Short C_SHORT

### Symbol :

### Illustration :

### Parameters :

> L = Length of transmission line connected to the coplanar short end.
> WG = Width of the ground plane at the shorted end (WG=0 ® infinite ground plane)
> C_LTYP = ID of coplanar transmission line applied at port 1
> C_SUB = ID of coplanar substrate definition
> C_GRID = ID of simulation control data
> TEMP = ID of element temperature definition used for noise computation

### Range of Usage :

> WG = 0.5.n.DL* n=1,2,3,...
> * ) see C_GRID for information on DL

### Notes/Equations/References :

> 1. The C_SHORT module represents a short circuited coplanar line. The dimensions of the line connected to the short are defined using data item addressed by C_ LTYP. L is the length of the connected coplanar line.
> 2. WG is the extension of the ground plane at the end of shorted line.
> 3. A negative value for L can be meaningful during the simulation. In such cases, the automated layout generation works incorrectly and the generated layout has to be edited manually. The minimum value for L depends on the metal layer oversizes in the currently selected C_LAYER. In case of DEFAULT foundry, L should be greater than or equal to max(|cond_os|, |cond2_os|).
> 4. For WG =0, infinite ground plane at the shorted end is assumed for the simulation.
> 5. If L1 and L2 in selected C_GRID are not set to -1 (auto sizing), the minimum values for L1 and L2 are:
>    L1min=W+2*S+2*GW
>    L2min=8*DL{C_GRID}+WG
> 6. See notations in chapter 4 (Important Note!) for the correct selection of the C_LTYP.

### Equivalent Circuit :

> For the modeling of the C_SHORT element, an equivalent inductance is used. The value of this inductance is derived from quasi-static FD-calculations. The connected line at the port is modeled as a C_LIN element and is represented by its characteristic impedance ZL and phase constant b. There is no limitation due to the length of connected line (L).

### Layout :

> 1. 1. For L=0 only the ground plane at the end of line is drawn.
> 2. 2. If CEN_MET and GND_MET in the selected C_LTYP are at different levels, the ground plane at shorted end is built in both metal level .
> 3. 3. If the parameter GW_DEF in C_PROCES is set to a positive non-zero value, this value is used as ground width for layout generation.

[to index] | [close window] | [C_SHORT Verification]