[close window] | [C_RIND]

# Coplanar Rectangular Inductor C_RIND

### Notes :

> The simulation of the first two test circuits have been made utilizing the quasi static Finite Difference formulation (indicated with sim) and the full wave Finite Difference Time Domain analysis (indicated with fdtd).

Configuration: 50W1 CPW lines with airbridges of TYPE=2, BW=50mm, BS=14mm, bg=8mm feed line length = 400mm inductor configuration:N = 1.5, WF=25mm, SF=20mm, IDIA1=95mm, IDIA2=50mm, S=30mm, BW=25mm, BS=14mm, BG=8mm |

Configuration: 50W1 CPW lines with airbridges of TYPE=2, BW=50mm, BS=14mm, BG=8mm feedline length = 400mm inductor configuration:N = 3.5, WF=8mm, SF=7mm, IDIA1=92mm, IDIA2=77mm, S=33.5mm, BW=8mm, BS=14mm, BG=8mm |

Configuration: 50W CPW lines (W=50, S=40, D=50mm) inductor configuration: N = 9.5, WF=10mm, SF=8mm, IDIA1=125mm, IDIA2=108mm, S=20mm, BW=10mm, BS=10mm, BG=10mm |

[close window] | [C_RIND]