[close window] | [C_LIN]

# Coplanar Transmission Line C_LIN

### Notes :

> These 'long lines' have been realized to determine the losses of different coplanar line configuration. Note, that the S-matrix is always normalized to 50W. The circuit has to be simulated with the elements C_OPEN as a termination of C_LIN, because the calibration was made on a substrate with abrupt ending coplanar lines. An other enhancement of the calculated results can be achieved, when we take an offset of the probe tips position to the desired ports into account.

Configuration: 40W5 CPW line terminated with shorted ground strips at each end of the line. |

Configuration: 50W1 CPW configuration |

Configuration: 60W6 CPW configuration |

[close window] | [C_LIN]